**General**

The machine is suitable for cleaning of vegetables, fruits, seafood, products and other granules and rootstock products. For ex

**Technical parameter**

|  |  |
| --- | --- |
| **Processing capacity** | 500~1500kg/h |
| **Power:** | 3.3 kw |
| **Water consumption:** | 0.5~1.0 t/h (Circulating water) |
| **Overall size:** | 5380×1550×1230mm |

